Updating the Hybrid Clock is easy..

- Use the Access Point of the Hybrid Clock by switching WIFI to AP in the MENU
- Press CONF to start the Access Point
- Connect your computer the Wifi-network "HybridClock" - password "987654321xx"
- Go to 192.168.4.1 with your browser
- Click Firmware Update, select the .bin file in this folder
- Click update and wait till the update is finished

If updating from a firmware before 1.5 add the following steps..

- Start CONF again
- Go to 192.168.4.1 with your browser
- Click RESET to reset all to default
- Calibrate the potentiometers

Have fun!
